**New installation**

**Using a USB thumb drive**

1. Copy 7E\_universal\_V1.xx.exe onto a computer.

2. Execute 7E\_universal\_V1.xx.exe on the same computer.

3. Insert a USB thumb drive into the computer.

4. Follow the instructions on the screen.

5. Plug the USB thumb drive into the 7E / 7Ex / ES-versa.

6. Start the 7E / 7Ex / ES-versa.

7. Follow the instructions on the screen

**Using a Floppy disk**

1. Copy 7E\_universal\_V1.xx.exe onto a computer.

2. Execute 7E\_universal\_V1.xx.exe on the same computer.

3. Insert a floppy disk into the computer.

4. Follow the instructions on the screen.

5. Insert the floppy disk into the 7E / 7Ex / ES-versa.

6. Start the 7E / 7Ex / ES-versa.

7. Follow the instructions on the screen.

**Updates**

Follow the instructions as for “New installation”.